139 Acadian Lane

Mandeville, Louisiana 70471

`	(985)845-9829/(504)430-7117

Harris B. Doucet

9000 HORSEPOWER CLASS
OFFICIAL NUMBER – 560405
IMO NUMBER ‐7367249
MAIN IRON WORKS - YEAR BUILT – 1974 /
YEAR RE‐BUILT ‐ 1998

DIMENSIONS	PROPULSION
Length	120’	Engine Make	(2) EMD
Width	34’	Engine Model	12‐645‐E5
Depth	16’	Reduction Gear Make	Lufkin
Draft – Min.	14.5’	Reduction Gear Model	5.02:1
Draft – Max.	16’	Propellers	111 in. X 118 in. in Kort Nozzle
4 Blade Stainless Steel
CALL SIGN	WAK 8008	Controls	Schrader Bellows
Steering	Racine
HULL CHARACTERISTICS
Gross Tonnage	ITC – 437 / GRT – 98	BOLLARD PULL:	66.88 Short Tons ABS Certified
Net Tonnage	ITC – 131 / NRT – 66
CAPACITIES
GENERATORS	Fuel	100,000 gallons
Make	(2) John Deere	Water	18,000 gallons
Model	6.8 liter tier 2, 99KW	Lube oil	2,800 gallons
NAVAGATION/COMMUNICATION EQUIPMENT	LIVING QUARTERS
Radar (2), Fathometer, Auto Pilot, VHF Radio (3), GPS,	Bunks	13
Single Sideband Radio, Satellite Telephone,	Heads	2
Cell phone, EPIRB, SatNav, Fax, e‐mail	Showers	2
CERTIFICATES	TOWING WINCH
Certificate of Documentation	Make	Smatco Double Drum
ABS Classed A‐1 Towing Service, AMS	Towing Drum	2,500 ft. of 2‐1/4 in. cable
ISM Certified	Anchor Drum

(All details and specifications as per Owner and not guaranteed by Broker.)